**How to Install Zest Wall and Shower Panels**

Zest wall panels are quick and easy to install creating minimal disruption, particularly compared to the time consuming alternative of tiling.

Below you will find helpful hints, as well as a comprehensive step-by-step guide on how to install your new Zest wall panels. We hope the following advice will help guide you through the installation and care of your new Zest wall panels.

**Boards fitted to flat, dry walls and ceilings.**

**Installation process for Zest Wall Panels:`**

**Step 1**

Select and fit trims required.

**Step 2**

Select the first panel and cut to length. Remember, if the last panel in the run is on a feature corner, you could remove more of the first panel to finish with a complete panel.

**Step 3**

Painted surfaces should be suitably keyed before applying any adhesive.

**Step 4**

Apply adhesive evenly to the surface of the wall, or rear of panel, in a zigzag pattern.

**Step 5**

Starting from the left, fit the panel into the trim using a spirit level to ensure the panel is vertical.

**Step 6**

Make sure the panel is securely bonded to the wall.

**Step 7**

When fixing to tiled walls use a neutral cure silicone or solvent free/moisture cure adhesive.